Sensor: GeoEye-1
Acquired Nominal GSD
   Pan Cross Scan: 0.4360632002 meters
   Pan Along Scan: 0.4332652092 meters
   MS Cross Scan: 1.7442528009 meters
   MS Along Scan: 1.7330608368 meters
Scan Azimuth: 269.8866163553 degrees
Scan Direction: Reverse
Panchromatic TDI Mode: 32
Multispectral TDI Mode13: 14
Multispectral TDI Mode24: 10
Camera Cal Creation DateTime: 2011-10-03 17:03:28 GMT
Ancillary Cal Creation DateTime: 2011-04-29 21:39:10 GMT
Gain Cal Creation DateTime: 2009-09-18 21:35:03 GMT
Dark Offset Cal Creation DateTime: 2009-09-18 21:35:03 GMT
Camera Cal Effective DateTime: 2049-11-30 00:00:00 GMT
Ancillary Cal Effective DateTime: 2011-03-26 00:00:00 GMT
Gain Cal Effective DateTime: 2009-07-29 00:00:00 GMT
Dark Offset Cal Effective DateTime: 2009-07-29 00:00:00 GMT
Pan Line Rate: 10000
Nominal Collection Azimuth: 42.3288 degrees
Nominal Collection Elevation: 76.03703 degrees
Sun Angle Azimuth: 163.7740 degrees
Sun Angle Elevation: 16.62766 degrees
Acquisition Date/Time: 2012-02-04 08:38 GMT
Percent Cloud Cover: 4

