/*! \page gpdelib GRASS partial differential equations Library (GPDE)

<h2>GRASS Partial Differential Equations Library (GPDE)</h2>

<P>
Author: Soeren Gebbert

<b>Overview</b>

The GRASS partial differential equation library is designed to support the
solution of PDE's within GRASS.
Therefore it provides functions to create and solve linear equation systems.
The library design is thread safe and supports threaded parallelism with OpenMP. 
Most of the available solvers (expect the gauss seidel and jacobi solver)
and the assembling of the linear equation systems are parallelized with OpenMP. 
The creation of a linear equation system can be done by using quadratic or sparse matrices.
Sparse and quadratic matrices are supported by the iterative equation solvers, 
the direct equation solvers only support regular quadratic matrices.
<p>
To enable parallel computing, you will need a compiler with OpenMP capabilities
and a computer with at least two cores or cpu's.
Most proprietary compilers support OpenMP. 
The free gnu-C compiler supports OpenMP since version 4.2.
More informations about OpenMP are available at http://www.openmp.org .
<br>
<br>
Based on the finite volume discretization for structured grids, 
groundwater flow and solute transport in 2d and 3d are implemented. 
It is IMHO easy to add any partial differential equation which can be 
solved with the finite volume or the finite differences method based on structured grids.
The basis for the discretisation is the geometrical structure of raster and volume maps.
<br>
<br>
There are plans to implement heat flow in two and three dimensions.
<br>
<br>
Currently only planimetric projections are supported for numerical calculations.
<br>
<br>
The gpde library provides an easy to handle interface for reading raster and volume data into
specific data arrays (in memory) and for writing data arrays to raster and volume maps. 
These data arrays supports all raster and volume datatypes, overlapping boundaries 
and provide a sophisticated null value support and array access functions. 
Basic mathematical operations are available for the arrays.

\section PDE The Creation of a lineare equation systems

The principle to create and solve a linear equation systems with this library:
\verbatim
1.) Read all needed raster/volume data into the memory
    - use the the two and three dimensional data arrays N_array_2d and N_array_3d
      to manage the data
2.) Assemble the linear equation system
    - use the sparse matrix structure to save lots of memory and cpu time
3.) Solve the linear equation system with the gauss, lu, jacobi, sor, cg or bicgstab method
    - always prefer the iterative krylov-space methods for solving
    - if the linear equation systems are in a bad condition try the jacobian solver
    - the available direct solvers dont support sparse matrices
4.) Write the result back as raster/volume map
\endverbatim

The following code shows how to implement this principle with the GRASS PDE lib:

\verbatim
/* *************************************************************** */
/* ****** calculate 2d dimensional groundwater flow ************** */
/* *************************************************************** */
int main()
{
    int i, j;
    N_gwflow_data2d *data = NULL; 	/* data structure with the groundwater data		*/
    N_geom_data *geom = NULL; 		/* geometry of the calculation area (region)		*/
    N_les *les = NULL; 		/* the linear equation system structure			*/
    N_les_callback_2d *call = NULL;	/* the callback for the groundwater flow calulation	*/

    /* allocate the callback structure */
    call = N_alloc_les_callback_2d();

    /* set the callback to groundwater flow calculation */
    N_set_les_callback_2d_func(call, (*N_callback_gwflow_2d));

   /* allocate the groundwater data structure with one million cells */
    data = N_alloc_gwflow_data2d(1000, 1000);

    /* get the current region */
    G_get_set_window(&region);

    /* allocate and initiate the geometry structure  for geometry and area calculation
       needed by the groundwater calculation callback */
    geom = N_init_geom_data_2d(&region, geom);

 
    /*fill the data arrays with raster maps*/
    N_read_rast_to_array_2d("phead_map_name", data->phead);      
    N_read_rast_to_array_2d("phead_map_name", data->phead_start);
    N_read_rast_to_array_2d("status_map_name", data->status);
    N_read_rast_to_array_2d("hc_x_map_name", data->hc_x);
    N_read_rast_to_array_2d("hc_y_map_name", data->hc_y);
    N_read_rast_to_array_2d("q_map_name", data->q);
    N_read_rast_to_array_2d("s_map_name", data->s);
    N_read_rast_to_array_2d("top_map_name", data->top);
    N_read_rast_to_array_2d("bottom_map_name", data->bottom);
    N_read_rast_to_array_2d("r_map_name", data->r);

    /* Set the inactive cells to zero, to assure a no flow boundary */
    /* notice: the data arrays are of type DCELL, so the put_*_d_value functions are used */
    for (y = 0; y < geom->rows; y++) {
	for (x = 0; x < geom->cols; x++) {
	    stat = (int)N_get_array_2d_d_value(data->status, x, y);
	    if (stat == N_CELL_INACTIVE) {	/*only inactive cells */
		N_put_array_2d_d_value(data->hc_x, x, y, 0);
		N_put_array_2d_d_value(data->hc_y, x, y, 0);
		N_put_array_2d_d_value(data->s, x, y, 0);
		N_put_array_2d_d_value(data->q, x, y, 0);
	    }
	}
    }
 
    /*Assemble the sparse matrix */
    les = N_assemble_les_2d(N_SPARSE_LES, geom, data->status, data->phead_start, (void *)data, call);

    /*Solve the linear equation system with the cg method*/
    N_solver_cg(les, 100000, 0.1e-8);

    /* now copy the result from the x vector of the linear equation system
       into a data array, this function is not provided by the gpde lib, 
       you have to write your own: take a look at r.gwflow 
    */
    copy_x_vect_to_data_array(les->x, data->phead, geom);

    /*write the x vector of the les back into a raster map*/
    N_write_array_2d_to_rast(data->phead, "output_map_name");

    /*free the memory*/
    N_free_les(les);
    N_free_gwflow_data2d(data);
    N_free_geom_data(geom);
    G_free(call);

    return 0;
}

\endverbatim

The assembling of lineare equation systems is based on a 5 point star for raster maps and a
7 point star for volume maps, implemented as finite volume/differences discretization. 

<p>
All raster and volume maps which are used to create a linear equation system
must be loaded completely into the memory.<br>
Therefore 2d and 3d data structures are implemented to support this principle:

\subsection rastermaps Raster maps

\verbatim

This structure manages two dimensional data 

typedef struct
{
    int type;                   /* which raster type CELL_TYPE, FCELL_TYPE, DCELL_TYPE */
    int rows, cols;
    int rows_intern, cols_intern;
    int offset;                 /*number of cols/rows offset at each boundary */
    CELL *cell_array;
    FCELL *fcell_array;
    DCELL *dcell_array;
} N_array_2d;
\endverbatim

For performance reasons the data arrays are stored as a one dimensional array internally.<br>
Use the following functions for memory allocation and value handling:
<p>
Memory allocation<br>
N_array_2d *#N_alloc_array_2d(int rows, int cols, int offset, int type);
<p>
void #N_free_array_2d(N_array_2d * data_array);
<p>
Get the type of the array<br>
int #N_get_array_2d_type(N_array_2d * array2d);
<p>
To access the 2d arrays use the following functions for reading and writing of data values
<p>
void #N_get_array_2d_value(N_array_2d * array2d, int row, int col, void *value);
<p>
CELL #N_get_array_2d_c_value(N_array_2d * array2d, int row, int col);
<p>
FCELL #N_get_array_2d_f_value(N_array_2d * array2d, int row, int col);
<p>
DCELL #N_get_array_2d_d_value(N_array_2d * array2d, int row, int col);
<p>
void #N_put_array_2d_value(N_array_2d * array2d, int row, int col, char *value);
<p>
void #N_put_array_2d_c_value(N_array_2d * array2d, int row, int col, CELL value);
<p>
void #N_put_array_2d_f_value(N_array_2d * array2d, int row, int col, FCELL value);
<p>
void #N_put_array_2d_d_value(N_array_2d * array2d, int row, int col, DCELL value);
<p>
\subsubsection highlevel Higher level array functions

To copy one array to another use this function<br>

void #N_copy_array_2d(N_array_2d * source, N_array_2d * target);
<p>
Print the content of the array to stdout<br>
void #N_print_array_2d (N_array_2d * data);
<p>
Compute the norm of two arrays<br>
double #N_norm_array_2d (N_array_2d * array1, N_array_2d * array2, int type);
<p>
Performe some basic mathematical operations with two arrays<br>
N_array_2d * #N_math_array_2d (N_array_2d * array1, N_array_2d * array2, N_array_2d * result, int type);
<p>
Convert all null values to zero<br>
int #N_convert_array_2d_null_to_zero (N_array_2d * a);
<p>
Read a raster map into the memory<br>
N_array_2d * #N_read_rast_to_array_2d (char *name, N_array_2d * array);
<p>
Write a raster map to the disk<br>
void #N_write_array_2d_to_rast (N_array_2d * array, char *name);

<P>
<b>Example implementation:</b><br>
The GRASS module <a href="http://grass.osgeo.org/grass63/manuals/html63_user/r.gwflow.html">r.gwflow</a>
implements numerical calculation program for transient,
confined and unconfined groundwater flow in two dimensions.

\subsection g3dmaps Volume maps
\verbatim
typedef struct
{

This structure manages three dimensional data 

    int type;                   /* which raster type FCELL_TYPE, DCELL_TYPE */
    int rows, cols, depths;
    int rows_intern, cols_intern, depths_intern;
    int offset;                 /*number of cols/rows/depths offset at each boundary */
    float *fcell_array;
    double *dcell_array;
} N_array_3d;
\endverbatim
For performance reasons the data arrays are stored as a one dimensional array internally.

<br><br>
The following functions should be used for memory allocation and value handling:
<p>
N_array_3d *#N_alloc_array_3d(int depths, int rows, int cols, int offset, int type);
<p>
void #N_free_array_3d(N_array_3d * data_array);
<p>
int #N_get_array_3d_type(N_array_3d * array);
<p>
To access the 3d arrays use the following functions for reading and writing of data values
<p>
void #N_get_array_3d_value(N_array_3d * array3d, int depth, int row, int col, void *value);
<p>
float #N_get_array_3d_f_value(N_array_3d * array3d, int depth, int row, int col);
<p>
double #N_get_array_3d_d_value(N_array_3d * array3d, int depth, int row, int col);
<p>
void #N_put_array_3d_value(N_array_3d * array3d, int depth, int row, int col, char *value);
<p>
void #N_put_array_3d_f_value(N_array_3d * array3d, int depth, int row, int col, float value);
<p>
void #N_put_array_3d_d_value(N_array_3d * array3d, int depth, int row, int col, double value);
<p>
\subsubsection highlevel Higher level array functions

To copy one array to another use this function
<br>
void #N_copy_array_3d(N_array_3d * source, N_array_3d * target);
<p>
Print the content of the array to stdout<br>
void #N_print_array_3d (N_array_3d * data);
<p>
Compute the norm of two arrays<br>
double #N_norm_array_3d (N_array_3d * array1, N_array_3d * array2, int type);
<p>
Performe some basic mathematical operations with two arrays<br>
N_array_3d * #N_math_array_3d (N_array_3d * array1, N_array_3d * array2, N_array_3d * result, int type);
<p>
Convert all null values to zero<br>
int #N_convert_array_3d_null_to_zero (N_array_3d * a);
<p>
Read a volume map into the memory<br>
N_array_3d * #N_read_rast3d_to_array_3d (char *name, N_array_3d * array, int mask);
<p>
Write a volume map to the disk<br>
void #N_write_array_3d_to_rast3d (N_array_3d * array, char *name, int mask);
<p>

<P>
<b>Example implementation:</b><br>
The GRASS module <a href="http://grass.itc.it/grass63/manuals/html63_user/r3.gwflow.html">r3.gwflow</a>
implements numerical calculation program for transient, confined
groundwater flow in three dimensions.


\subsection les Entries in the linear equation system

To make entries in the linear equation system, a special structure must be provided.
Currently implemented structures includes the 5 point and 7 point star scheme:

\verbatim
Matrix entries for the mass balance of a 5 star system

The entries are center, east, west, north, south and the
right side vector b of Ax = b. This system is typical used in 2d.

     N
     |
 W-- C --E
     |
     S

Matrix entries for the mass balance of a 7 star system

The entries are center, east, west, north, south, top, bottom and the
right side vector b of Ax = b. This system is typical used in 3d.

     T N
     |/
 W-- C --E
    /|
   S B

Matrix entries for the mass balance of a 9 star system

The entries are center, east, west, north, south, north-east, south-east,
north-wast, south-west and the
right side vector b of Ax = b. This system is typical used in 2d.

 NW  N  NE
   \ | /
 W-- C --E
   / | \
 SW  S  SE


typedef struct
{
    int type;
    int count;
    double W, E, N, S, C, T, B, NE, NW, SE, SW, V;
} N_data_star;
\endverbatim

The following functions should be used to create and handle the N_data_star structures:

<p>
Memory allocation<br>
N_data_star *#N_alloc_5star(void);
<p>
N_data_star *#N_alloc_7star(void);
<p>
N_data_star *#N_alloc_9star(void);
<p>
Memory allocation with initialisation<br>
N_data_star *#N_create_5star(double C, double W, double E, double N, double S, double V);
<p>
N_data_star *#N_create_7star(double C, double W, double E, double N, double S, double T, double B, double V);
<p>
N_data_star *#N_create_9star(double C, double W, double E, double N, double S, double NW, double SW, double NE, double SE, double V);
<p>

<p>
\subsection les functions to assemble the lineare equation system

<p>
Setting the callback function which fills the 5 or 7 point structure for every row of the linear equation system (eg: for each cell of the raster or volume map)
<p>
void #N_set_les_callback_3d_func(N_les_callback_3d * data, N_data_star * (*callback_func_3d) ());
<p>
void #N_set_les_callback_2d_func(N_les_callback_2d * data, N_data_star * (*callback_func_2d) ());
<p>
Allocation the callback structure for 2d and 3d
<p>
N_les_callback_3d *#N_alloc_les_callback_3d(void);
<p>
N_les_callback_2d *#N_alloc_les_callback_2d(void);

<p>
Assemble the linear equation system in 2d or 3d

<p>
N_les *#N_assemble_les_3d(int les_type, N_geom_data * geom, N_array_3d * status, N_array_3d * start_val, void *data, N_les_callback_3d * callback);
<p>
N_les *#N_assemble_les_2d(int les_type, N_geom_data * geom, N_array_2d * status, N_array_2d * start_val, void *data, N_les_callback_2d * callback);

<p>
templates for callback functions
<p>
N_data_star *#N_callback_template_3d(void *data, N_geom_data * geom, int depth, int row, int col);
<p>
N_data_star *#N_callback_template_2d(void *data, N_geom_data * geom, int row, int col);


\section solvers Available solvers

\subsection direct_solvers Direct solvers

Two direct solvers are implemented, the gauss elimination solver and the lu decomposition solver.
The direct solvers only work with regular quadratic matrices, not with sparse matrices.

<p>
int #N_solver_gauss (N_les * les);

<p>
int #N_solver_lu (N_les * les);


\subsection iterative_solvers Iterative solvers 

The iterative solvers work with regular quadartic and sparse matrices.
<p>
To solve symmetric and positive definite linear equation systems the iterative 
conjugated gradient method with additional diagonal preconditioning are implemented.

int #N_solver_cg(N_les * les, int maxit, double error);
<p>
int #N_solver_pcg(N_les * les, int maxit, double error);

<p>
To solve unsymmetric non definite linear equation system the iterative BiCGSatb method is implemented

<p>
int #N_solver_bicgstab(N_les * les, int maxit, double error);

<p>
Additionally jacobi and Gauss-Seidel iterative solvers with relaxation are implemented
<p>
int #N_solver_jacobi (N_les * L, int maxit, double sor, double error);
<p>
int #N_solver_SOR (N_les * L, int maxit, double sor, double error);

\section available_pdes Implemented PDE's

Groundwater flow in 2 and 3 dimensions are implemented.


This data structure contains all data needed to compute the 
groundwater mass balance in three dimension 

\verbatim
typedef struct
{
  N_array_3d *phead;		/*!piezometric head */
  N_array_3d *phead_start;	/*!start conditions */
  N_array_3d *hc_x;		/*!x part of the hydraulic conductivity tensor */
  N_array_3d *hc_y;		/*!y part of the hydraulic conductivity tensor */
  N_array_3d *hc_z;		/*!z part of the hydraulic conductivity tensor */
  N_array_3d *q;		/*!sources and sinks */
  N_array_2d *r;		/*!recharge at the top of the gw leayer */
  N_array_3d *s;		/*!specific yield */
  N_array_3d *nf;		/*!effective porosity */

  N_array_3d *status;		/*!active/inactive/dirichlet cell status */

  double dt;			/*!calculation time */

} N_gwflow_data3d;
\endverbatim


This data structure contains all data needed to compute the 
groundwater mass balance in two dimension 

 \verbatim
typedef struct
{
  N_array_2d *phead;		/*!piezometric head */
  N_array_2d *phead_start;	/*!start conditions */
  N_array_2d *hc_x;		/*!x part of the hydraulic conductivity tensor */
  N_array_2d *hc_y;		/*!y part of the hydraulic conductivity tensor */
  N_array_2d *q;		/*!sources and sinks */
  N_array_2d *r;		/*!recharge at the top of the gw leayer */
  N_array_2d *s;		/*!specific yield */
  N_array_2d *nf;		/*!effective porosity */

  N_array_2d *top;		/*!top surface of the quifer */
  N_array_2d *bottom;		/*!bottom of the aquifer */

  N_array_2d *status;		/*!active/inactive/dirichlet cell status */

  double dt;			/*!calculation time */
  int gwtype;			/*!Which type of groundwater, N_GW_CONFINED or N_GW_UNCONFIED */

} N_gwflow_data2d;
\endverbatim

<p>
The callback to compute a les row entry in 3d dimesnions<br>
N_data_star *#N_callback_gwflow_3d (void *gwdata, N_geom_data * geom, int col, int row, int depth);
<p>
The callback to compute a les row entry in 2d dimesnions<br>
N_data_star *#N_callback_gwflow_2d (void *gwdata, N_geom_data * geom, int col, int row);
<p>
Allocation the 3d groundwater flow data structure<br>
N_gwflow_data3d *#N_alloc_gwflow_data3d (int cols, int rows, int depths);
<p>
Allocation the 2d groundwater flow data structure<br>
N_gwflow_data2d *#N_alloc_gwflow_data2d (int cols, int rows);
<p>
Releasing memory<br>
void #N_free_gwflow_data3d (N_gwflow_data3d * data);
<p>
Releasing memory<br>
void #N_free_gwflow_data2d (N_gwflow_data2d * data);
<p>

\section geom_data Handling geometrical data

To handle geometrical data a special data structure was implemented.<br>


\verbatim
Geometric informations about the structured grid is stored in this structure

typedef struct
{
  int planimetric; /*If the projection is not planimetric (0), the array calculation is different for each row*/
  double *area; /* the vector of area values for non-planimetric projection for each row*/
  int dim; /* 2 or 3*/

  double dx;
  double dy;
  double dz;

  double Az;

  int depths;
  int rows;
  int cols;

} N_geom_data;
\endverbatim

Use the follwoing functions to handle the geometric data structures:

<p>
Creating a N_geom_data structure<br>
N_geom_data *#N_alloc_geom_data (void);
<p>
Releasing memory<br>
void #N_free_geom_data (N_geom_data *geodata);
<p>
Initialize the N_geom_data structure with a G3D_Region<br>
N_geom_data *#N_init_geom_data_3d(G3D_Region * region3d, N_geom_data * geodata);
<p>
Initialize the N_geom_data structure with a 2d region<br>
N_geom_data *#N_init_geom_data_2d(struct Cell_head * region, N_geom_data * geodata);
<p>
Get the area of a cell in row<br>
double #N_get_geom_data_area_of_cell(N_geom_data * geom, int row);

\section mathtools Mathematical tools

Several mean calculation algorithms are implemented.
Two versions of each algorithm are available working 
with two values or a vector of values.

<p>
double #N_calc_arith_mean(double a, double b)
<p>
double #N_calc_arith_mean_n(double *a, int size)
<p>
double #N_calc_geom_mean(double a, double b)
<p>
double #N_calc_geom_mean_n(double *a, int size)
<p>
double #N_calc_harmonic_mean(double a, double b)
<p>
double #N_calc_harmonic_mean_n(double *a, int size)
<p>
double #N_calc_quad_mean(double a, double b)
<p>
double #N_calc_quad_mean_n(double *a, int size)
<p>

Two methods for upwinding stabilization are implemented.

double #N_full_upwinding(double vector, double distance, double D)
<p>
double #N_exp_upwinding(double vector, double distance, double D)



\section gradient Calculating and managing gradient and vector field data

To compute and manage gradient and vector field data, specific data structures with access and management functions
are implemented. Gradient and vector field data is often needed in transport calculation like solute/heat transport
or navier stokes equations. The following  structures and functions provide a concient way to performe 
gradient and vector field calculations.
<p>

The gradient of one cell to there neighbours in each direction has the following components:

\verbatim

The two dimensional gradient consits of 4 values between the neighbour cells
 ______________ 
|    |    |    |
|    |    |    |
|----|-NC-|----|
|    |    |    |
|   WC    EC   |
|    |    |    |
|----|-SC-|----|
|    |    |    |
|____|____|____|

The three dimensional gradient consits of 6 values between the neighbour cells

      |  /
     TC NC
      |/
--WC-----EC--
     /|
   SC BC
   /  |

\endverbatim

Gradient between the cells in X and Y direction 

\verbatim
typedef struct {

  double NC, SC, WC, EC;

} N_gradient_2d;
\endverbatim

Gradient between the cells in X, Y and Z direction
\verbatim
typedef struct {

  double NC, SC, WC, EC, TC, BC;

} N_gradient_3d;
\endverbatim

The gradients between the neighbours of the center cell is needed for tensor 
calculation in the discretization of several partial differential equations.

\verbatim

Gradient in X direction between the cell neighbours
 ____ ____ ____
|    |    |    |
|   NWN  NEN   |
|____|____|____|
|    |    |    |
|   WN    EN   |
|____|____|____|
|    |    |    |
|   SWS  SES   |
|____|____|____|

Gradient in Y direction between the cell neighbours
 ______________ 
|    |    |    |
|    |    |    |
|NWW-|-NC-|-NEE|
|    |    |    |
|    |    |    |
|SWW-|-SC-|-SEE|
|    |    |    |
|____|____|____|

Gradient in Z direction between the cell neighbours
 /______________/
/|    |    |    |
 | NWZ| NZ | NEZ|
 |____|____|____|
/|    |    |    |
 | WZ | CZ | EZ |
 |____|____|____|
/|    |    |    |
 | SWZ| SZ | SEZ|
 |____|____|____|
/____/____/____/


\endverbatim

Gradient between the cell neighbours in X direction 

\verbatim
typedef struct {

  double NWN, NEN, WC, EC, SWS, SES;

} N_gradient_neighbours_x;
\endverbatim

Gradient between the cell neighbours in Y direction

\verbatim
typedef struct {

  double NWW, NEE, NC, SC, SWW, SEE;

} N_gradient_neighbours_y;
\endverbatim

Gradient between the cell neighbours in Z direction

\verbatim
typedef struct {

  double NWZ, NZ, NEZ, WZ, CZ, EZ, SWZ, SZ, SEZ;

} N_gradient_neighbours_z;
\endverbatim


Gradient between the cell neighbours in X and Y direction

\verbatim
typedef struct {

  N_gradient_neighbours_x *x;
  N_gradient_neighbours_y *y;

} N_gradient_neighbours_2d;
\endverbatim


Gradient between the cell neighbours in X, Y and Z direction

\verbatim
typedef struct {

  N_gradient_neighbours_x *xt; /*top values*/
  N_gradient_neighbours_x *xc; /*center values*/
  N_gradient_neighbours_x *xb; /*bottom values*/

  N_gradient_neighbours_y *yt; /*top values*/
  N_gradient_neighbours_y *yc; /*center values*/
  N_gradient_neighbours_y *yb; /*bottom values*/

  N_gradient_neighbours_z *zt; /*top-center values*/
  N_gradient_neighbours_z *zb; /*bottom-center values*/

} N_gradient_neighbours_3d;
\endverbatim


Two dimensional gradient field

\verbatim
typedef struct {

  N_array_2d *x_array;
  N_array_2d *y_array;

} N_gradient_field_2d;
\endverbatim

Three dimensional gradient field

\verbatim
typedef struct {

  N_array_3d *x_array;
  N_array_3d *y_array;
  N_array_3d *z_array;

} N_gradient_field_3d;

\endverbatim

Use the following functions for allocation and data handling:
<p>
Functions to handle a 2d gradient
<p>
N_gradient_2d * #N_alloc_gradient_2d(void);
<p>
void #N_free_gradient_2d(N_gradient_2d * grad);
<p>
N_gradient_2d * #N_create_gradient_2d(double NC, double SC, double WC, double EC);
<p>
int #N_copy_gradient_2d(N_gradient_2d * source, N_gradient_2d *target);
<p>
N_gradient_2d * #N_get_gradient_2d(N_gradient_field_2d *field, N_gradient_2d * gradient, int col, int row);
<p>
<p>
Functions to handle a 2d gradient
<p>

N_gradient_3d * #N_alloc_gradient_3d(void);
<p>
void #N_free_gradient_3d(N_gradient_3d * grad);
<p>
N_gradient_3d * #N_create_gradient_3d(double NC, double SC, double WC, double EC, double TC, double BC);
<p>
int #N_copy_gradient_3d(N_gradient_3d * source, N_gradient_3d *target);
<p>
N_gradient_3d * #N_get_gradient_3d(N_gradient_field_3d *field, N_gradient_3d * gradient, int col, int row, int depth);
<p>
<p>
Functions to handle gradient neighbours in x direction of the center cell
<p>

N_gradient_neighbours_x  * #N_alloc_gradient_neighbours_x(void);
<p>
void #N_free_gradient_neighbours_x(N_gradient_neighbours_x  *grad);
<p>
N_gradient_neighbours_x  * #N_create_gradient_neighbours_x(double NWN, double NEN, double WC, double EC, double SWS, double SES);
<p>
int #N_copy_gradient_neighbours_x(N_gradient_neighbours_x * source, N_gradient_neighbours_x *target);
<p>
<p>
Functions to handle gradient neighbours in y direction of the center cell
<p>

N_gradient_neighbours_y  * #N_alloc_gradient_neighbours_y(void);
<p>
void #N_free_gradient_neighbours_y(N_gradient_neighbours_y *grad);
<p>
N_gradient_neighbours_y  * #N_create_gradient_neighbours_y(double NWW, double NEE, double NC, double SC, double SWW, double SEE);
<p>
int #N_copy_gradient_neighbours_y(N_gradient_neighbours_y * source, N_gradient_neighbours_y *target);
<p>
<p>
Functions to handle gradient neighbours in z direction of the center cell
<p>

N_gradient_neighbours_z  * #N_alloc_gradient_neighbours_z(void);
<p>
void #N_free_gradient_neighbours_z(N_gradient_neighbours_z  *grad);
<p>
N_gradient_neighbours_z  * #N_create_gradient_neighbours_z(double NWZ, double NZ, double NEZ, double WZ, double CZ, double EZ, 
 						  double SWZ, double SZ, double SEZ);
<p>
int #N_copy_gradient_neighbours_z(N_gradient_neighbours_z * source, N_gradient_neighbours_z *target);
<p>
<p>
Functions to handle a 2d gradient neighbour structure of the center cell
<p>

N_gradient_neighbours_2d * #N_alloc_gradient_neighbours_2d(void);
<p>
void #N_free_gradient_neighbours_2d(N_gradient_neighbours_2d *grad);
<p>
N_gradient_neighbours_2d * #N_create_gradient_neighbours_2d(N_gradient_neighbours_x *x, N_gradient_neighbours_y *y);
<p>
int #N_copy_gradient_neighbours_2d(N_gradient_neighbours_2d *source, N_gradient_neighbours_2d *target);
<p>

<p>
Functions to handle a 2d gradient neighbour structure of the center cell
<p>
N_gradient_neighbours_3d * #N_alloc_gradient_neighbours_3d(void);
<p>
void #N_free_gradient_neighbours_3d(N_gradient_neighbours_3d *grad);
<p>
int #N_copy_gradient_neighbours_3d(N_gradient_neighbours_3d *source, N_gradient_neighbours_3d *target);
<p>

<p>

<p>
To compute and handle a 2d gradient field the following functions are implemented:
<p>
N_gradient_field_2d * #N_alloc_gradient_field_2d(int cols, int rows);
<p>
void #N_free_gradient_field_2d(N_gradient_field_2d *field);
<p>
int #N_copy_gradient_field_2d(N_gradient_field_2d *source, N_gradient_field_2d *target);
<p>

The gradient is calculated between cells for each cell and direction.
The creation of a 2d gradient field is based on the following scheme:

\verbatim
  ______________ 
 |    |    |    |
 |    |    |    |
 |----|-NC-|----|
 |    |    |    |
 |   WC    EC   |
 |    |    |    |
 |----|-SC-|----|
 |    |    |    |
 |____|____|____|
 
 
 x - direction:
 
 r = 2 * weight[row][col]*weight[row][col + 1] / (weight[row][col]*weight[row][col + 1])
 EC = r * (pot[row][col] - pot[row][col + 1])/dx
 
 y - direction:
 
 r = 2 * weight[row][col]*weight[row + 1][col] / (weight[row][col]*weight[row + 1][col])
 SC = r * (pot[row][col] - pot[row + 1][col])/dy
 
 the values SC and EC are the values of the next row/col
\endverbatim
 

<p>
N_gradient_field_2d * #N_compute_gradient_field_2d(N_array_2d *pot, N_array_2d *weight_x, N_array_2d *weight_y, N_geom_data *geom, N_gradient_field_2d *gradfield);
<p>
The computation of the gradient vectors for each cell is based on this scheme
 \verbatim
  ______________ 
 |    |    |    |
 |    |    |    |
 |----|-NC-|----|
 |    |    |    |
 |   WC    EC   |
 |    |    |    |
 |----|-SC-|----|
 |    |    |    |
 |____|____|____|
 
 x vector component:
 
 x = (WC + EC) / 2
 
 y vector component:
 
 y = (NC + SC) / 2
 
 \endverbatim
<p>
void #N_compute_gradient_field_components_2d(N_gradient_field_2d *field, N_array_2d *x_comp, N_array_2d *y_comp);
<p>

<p>
N_gradient_field_3d * #N_alloc_gradient_field_3d(int cols, int rows, int depths);
<p>
void #N_free_gradient_field_3d(N_gradient_field_3d *field);
<p>
int #N_copy_gradient_field_3d(N_gradient_field_3d *source, N_gradient_field_3d *target);
<p>

The gradient is calculated between cells for each cell and direction.
The creation of a 2d gradient field is based on the following scheme:
 \verbatim

      |  /
     TC NC
      |/
--WC-----EC--
     /|
   SC BC
   /  |


 x - direction:
 
 r = 2 * weight_x[depth][row][col]*weight_x[depth][row][col + 1] / (weight_X[depth][row][col]*weight_x[depth][row][col + 1])
 EC = r * (pot[depth][row][col] - pot[depth][row][col + 1])/dx
 
 y - direction:
 
 r = 2 * weight_y[depth][row][col]*weight_y[depth][row + 1][col] / (weight_y[depth][row][col]*weight_y[depth][row + 1][col])
 SC = r * (pot[depth][row][col] - pot[depth][row + 1][col])/dy
 
 z - direction:
 
 r = 2 * weight_z[depth][row][col]*weight_z[depth + 1][row][col] / (weight_z[depth][row][col]*weight_z[depth + 1][row][col])
 TC = r * (pot[depth][row][col] - pot[depth + 1][row][col])/dy
 
 the values BC, NC, WC are the values of the next depth/row/col
 
 
 \endverbatim

<p>
N_gradient_field_3d *#N_compute_gradient_field_3d(N_array_3d * pot, N_array_3d * weight_x, N_array_3d * weight_y, N_array_3d * weight_z, N_geom_data * geom, N_gradient_field_3d *gradfield)
<p>
Based on this storages scheme the gradient vector for each cell is 
 calculated and stored in the provided  N_array_3d structures
 \verbatim
 
      |  /
     TC NC
      |/
--WC-----EC--
     /|
   SC BC
   /  | 
 
 x vector component:
 
 x = (WC + EC) / 2
 
 y vector component:
 
 y = (NC + SC) / 2
 
 z vector component:
 
 z = (TC + BC) / 2
 
 \endverbatim

<p>
N_compute_gradient_field_components_3d(N_gradient_field_3d * field, N_array_3d * x_comp, N_array_3d * y_comp, N_array_3d * z_comp)

*/
