photo.init

## NAME

photo.init

## DESCRIPTION

Aerial photographs may be either vertical or oblique. Vertical photographs can be truly vertical (nadir), or slightly tilted (less than 3 degree from the vertical). Usually aerial photos are tilted to some degree. We refer to the term vertical photograph up to a tilt of 3 degree.
Oblique aerial photographs are purposely taken with an angle between 3 and 90 degree from the nadir direction.

The use of photo.init (menu 6) is only required when rectifying a tilted or oblique aerial photo.

photo.init creates or modifies entries in a camera initial exposure station file for imagery group referenced by a sub-block. These entries include: the (XC,YC,ZC) standard (e.g. UTM) approximate coordinates of the camera exposure station; initial roll, pitch, and yaw angles (in degrees) of the cameras attitude; and the a priori standard deviations for these parameters. During the imagery program, photo.rectify, the initial camera exposure station file is used for computation of the ortho-rectification parameters. If no initial camera exposure station file exist, the default values are computed from the control points file created in photo.2target.

The following menu is displayed:

            Please provide the following information

    	INITIAL XC: Meters                __________
    	INITIAL YC: Meters                __________
    	INITIAL ZC: Meters                __________
    	INITIAL omega (roll) degrees:     __________
    	INITIAL phi  (pitch) degrees:     __________
    	INITIAL kappa  (yaw) degrees:     __________

    	Standard Deviation XC: Meters     __________
    	Standard Deviation YC: Meters     __________
    	Standard Deviation ZC: Meters     __________
    	Std. Dev. omega (roll) degrees:   __________
    	Std. Dev. phi  (pitch) degrees:   __________
    	Std. Dev. kappa  (yaw) degrees:   __________

            Use these values at run time? (1=yes, 0=no)

         AFTER COMPLETING ALL ANSWERS, HIT <ESC> TO CONTINUE
                      (OR <Ctrl-C> TO CANCEL)

The INITIAL values for (XC,YC,ZC) are expressed in standard (e.g. UTM) coordinates, and represent an approximation for the location of the camera at the time of exposure.

- X: East aircraft position;
- Y: North aircraft position;
- Z: Flight altitude above sea level

The INITIAL values for (omega,phi,kappa) are expressed in degrees, and represent an approximation for the cameras attitude at the time of exposure.

- Omega (roll): Raising or lowering of the wings (turning around the aircraft's axis);
- Phi (pitch): Raising or lowering of the aircraft's front (turning around the wings' axis);
- Kappa (yaw): Rotation needed to align the aerial photo to true north: needs to be denoted as +90 degree for clockwise turn and -90 degree for a counterclockwise turn.

The standard deviations for (XC,YC,ZC) are expressed in meters, and are used as a priori values for the standard deviations used in computation of the ortho rectification parameters.

The standard deviations for (omega,phi,kappa) are expressed in degrees, and are used as a priori values for the standard deviations used in computation of the ortho rectification parameters.

If Use these values at run time? (1=yes, 0=no) is set to 0, the values in this menu are not used.

## SEE ALSO

i.ortho.photo, photo.camera, photo.2image, photo.2target, photo.rectify

## AUTHOR

Mike Baba, DBA Systems, Inc.

Last changed: $Date: 2006-09-22 09:57:14 -0500 (Пт, 22 сен 2006) $